**Voltage tap M8 with fuse for busbars**

for measuring voltage tapping on busbars with existing M8 holes. For indoor use, conforms to IEC 60947-7-3.

Operating temperature: -10 to +55 °C

Relative humidity: 5 - 85 % (no condensation)

Protection class: IP20 (basic insulation)

Maximum voltage: 400 V AC

Test voltage: 3 kV / 50 Hz

Surge voltage: 6 kV 1.2 / 50 µs

Maximum operating current: 2 A

Voltage drop: < 500 mV AC

Fuse: 2 A, 450 V

Fuse tripping characteristic:F

Fuse dimensions: 5 x 25 mm

Fuse type: ceramic

Max. Short-circuit current: 70 kA

Max. Torque: 2.0 Nm

Colour: black

Primary connection (mm): 8

Cross-section of primary connection (mm²): 1.5 - 4

Dimensions (mm): 23.2 x 17

Weight (kg): 0,03

Delivery includes:

Mounting accessories, documentation, delivery, installation as well as connection.

Manufacturer: Janitza electronics

Type: ZK4 M8

Art.no.: 1011535