**Commissioning active filter**

incl. parameterisation, control measurement, report and instruction. The parameters, the filter performance and the before/after comparison must be documented in the report as part of the control measurement.

On the commissioning date, the filter must be installed ready for operation and normal load conditions (production operation) must be present.

Travel costs to and from the site as well as overnight stays will be charged at cost. Price group 4.

Manufacturer: Janitza electronics GmbH

Type: Service

Item no.: DL5101152