**1-phase compact residual current transformer splittable**

for retrofitting on cables / lines for operating current measurement.

Max. diameter round conductor: 8 mm

Detection: residual currents type A

Transformation ratio: 700 / 1

Residual current type: A according to IEC 60755

Residual current measuring range: 10 - 1000 mA

Accuracy class: 1

Protection class: IP 20

Dimensions: W:35 mm / H:35 mm / D:16 mm

Weight: 0.05 kg

Certification: UL, EN 61010-1

Approved and compatible for manufacturer's 20-channel operating and residual current monitor & memory.

Delivery included:

Matching of the design to the practical application (max. differential current, differential current type, mechanical design, etc.), burden & pre-convected connection cable 1.5m, delivery, mounting as well as connection to the measuring device.

Manufacturer: Janitza electronics GmbH

Type: SC-CT-21

Item no.: 1503084