**Single-phase energy meter MID 65A direct measurement S0**

Approval: MID / IEC

Connection: 65A / direct measurement

Dimensions in mm (HxWxD): 97x35x65

Weight (g): 140

Subunits: 2

Power dissipation voltage circuits: 1.0VA/0.4W total

Power dissipation current circuits: 0.007VA/0.007W per Ph.

Digital inputs for tariff switching

or for counting external pulses: 2

Digital outputs for active or reactive

reactive energy (S0) or alarm output: 1

Pulse frequency: 1-9999 imp/kWh

Pulse length: 10 - 990 ms

Operating temperature (°C): -40 to +70

Storage temperature (°C): -40 to +85

Protection class (front/terminals): IP51 / IP20

Max. conductor cross-section measurement (mm²): 25

Supply voltage: self-supplied

Voltage range (V AC): 1x 220 to 240V -20-+15%

Current range (A): 0.025 to 65

Frequency, fundamental (Hz): 50/60 -+5%

Measurement: 1-phase

Measurement accuracy active energy: Class 1 (B)

Measurement accuracy reactive energy: Class 2

Tariffs: 2

Communication interface: none

No reset of energy meter readings.

Meter is calibrated according to MID and approved according to IEC.

Make: Janitza electronics GmbH

Type: B21 311-10J

Item no. 1401353