**Commissioning of dynamic power controller**

incl. parameterisation, control measurement, report and instruction. The parameters, the compensation performance and the before/after comparison must be documented in the report as part of the control measurement.

On the commissioning date, the SVG must be installed ready for operation and normal load conditions (production operation) must be present.

Travel costs to and from the site as well as overnight stays will be charged at cost. Price group 4.

Manufacturer: Janitza electronics GmbH

Type: Service