**Voltage tap without fuse protection**

For tapping the measuring voltage of the multifunctional measuring devices by means of terminals on current-carrying rails without fuse protection.

Colour: blue

Cross-section of connecting measuring cable (mm²): 0 - 16

Weight (kg): 0.1

Dimensions (mm): 58.2 x 76

Max. Operating voltage: 690 V

Test voltage / pulse: 3 kV / 50 Hz 6 kV

Short-circuit resistance 70 kA at 400 V / 50 Hz

Rated operating current In: max. 10 A

Insulation class: E (max. 120°)

Fuse type: 5 x 25 mm (with detector), 10 A SIBA DIN 41576-2

Ambient temperature: -5 to +40 °C

Primary fuse inside:-socket head screw M8

Hexagon socket: Number 6

Max. Rail thickness: 4 - 15 mm

Housing: Polyamide (PA6.6)

Terminal material: Nickel-plated brass

Delivery includes:

Mounting accessories, documentation, delivery, assembly as well as connection.

Manufacturer: Janitza electronics

Type: ZK 4 B

Art.no.: 1011526