**1-phase compact bushing differential current transformer**

for monitoring outgoing feeders to loads for differential currents type A on 3-phase disconnectors with phase distance of 17.5 mm.

Max. diameter round conductor: 7.5 mm

Evaluation: operating or residual currents type A

Transformation ratio: 700 / 1

Operating current measuring range: 0 to 63 A with load

Residual current type: A according to IEC 60755

Residual current measuring range: 10 to 1000 mA

Accuracy class: 1

Protection class: E

Protection class: IP 20

Dimensions: W:27 mm / H:46 mm / D:23 mm

Weight: 0.05 kg

Approved and compatible for manufacturer's 20-channel & memory operating and residual current monitor.

Delivery included:

Matching of the design to the practical application (max. differential current, differential current type, mechanical design, etc.), burden & pre-convected connection cable 1.5m, delivery, mounting as well as connection to the measuring device.

Manufacturer: Janitza electronics GmbH

Type: CT-20

Item no.: 1503082