**Splittable operating current transformer 100A for multi-channel power analyser**

for retrofitting on cables / lines for operating current measurement.

Maximum operating current: 100 A

Max. Diameter round conductor: 16 mm

Transformation ratio: 3000 / 1

Measuring accuracy class:1

Installation location: Indoor use

Conductor type: Insulated conductors

Ambient temperature: -10 to +50 °C

Dimensions (HxWxD): approx. 55 x 29.5 x 31

Weight: 0.075 kg

Approved and compatible for manufacturer's 20-channel & memory operating and residual current monitor.

Delivery included:

Matching of the design to the practical application (max. differential current, differential current type, mechanical design, etc.), burden & pre-convected connection cable 1.5m, delivery, mounting as well as connection to the measuring device.

Manufacturer: Janitza electronics GmbH

Type: SC-CT-20-100

Item no.: 1503093