**Three-phase current transformer 75 / 5A**

for mounting on top-hat rail, in plastic housing.

Max. Diameter round conductor: 13 mm

Load capacity: 75A

Secondary: 5A

Accuracy class: 1

Power: 1.5 VA

Number of current transformer cores: 3

Dimensions in mm: W: 90, H: 105, D: 54 (6HP)

Delivery includes:

Measuring transformer disconnect terminals with screw connection 0.2 - 10 mm², bridges as well as DIN rail clamp for DIN rail mounting according to DIN VDE 0100 - 557.5.3.1., adjustment of the design to the practical application (primary & secondary current, mechanical design, power & cable length, etc.), delivery, assembly as well as connection to the measuring device.

Manufacturer: Janitza electronics GmbH

Type: ASRD 14

Item no. 1503404