**1-phase switching power supply unit for residual current transformers type B+**

in installation housing for supplying the manufacturer's residual current transformers type B+.

Primary voltage: 115 - 230 V AC

Rated frequency: 50 / 60 Hz

Secondary voltage: 24V DC

Secondary current 1 A

Approved and compatible with the manufacturer's differential current transformers requiring active supply voltage.

Delivery included:

Matching of the design to the practical application (max. differential current, differential current type, mechanical design, etc.), delivery, assembly as well as connection to the measuring device.

Manufacturer: Janitza electronics GmbH

Type: Power supply B+ converter

Art.no.: 1605002